**Source Code**

**Python Code**

#IBM Watson IOT Platform

#pip install wiotp-sdk

import wiotp.sdk.device

import time

import random

myConfig = {

"identity": {

"orgId": "14dcvs",

"typeId": "Device1",

"deviceId":"12345"

},

"auth": {

"token": "87654321"

}

}

def myCommandCallback(cmd):

print("Message received from IBM IoT Platform: %s" % cmd.data['command'])

m=cmd.data['command']

if(m=="Motor On"):

print("\*\*\*\*///Motors ARE ON///\*\*\*\*")

else:

print("\*\*\*\*///Motors ARE OFF///\*\*\*\*")

client = wiotp.sdk.device.DeviceClient(config=myConfig, logHandlers=None)

client.connect()

while True:

temp=random.randint(-20,125)

hum=random.randint(0,100)

Mois=random.randint(20,120)

myData={'temperature':temp, 'humidity':hum, 'moisture':Mois}

client.publishEvent(eventId="status", msgFormat="json", data=myData, qos=0, onPublish=None)

print("Published data Successfully: %s", myData)

client.commandCallback = myCommandCallback

time.sleep(2)

client.disconnect()

**Arduino Code In Wokwi:**

#include <WiFi.h>//library for wifi

#include <PubSubClient.h>//library for MQtt

#include "DHT.h"// Library for dht11

#define DHTPIN 15     // what pin we're connected to

#define DHTTYPE DHT22   // define type of sensor DHT 11

#define LED 2

DHT dht (DHTPIN, DHTTYPE);// creating the instance by passing pin and typr of dht connected

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "14dcvs"//IBM ORGANITION ID

#define DEVICE\_TYPE "Device1"//Device type mentioned in ibm watson IOT Platform

#define DEVICE\_ID "12345"//Device ID mentioned in ibm watson IOT Platform

#define TOKEN "87654321"     //Token

String data3;

float h, t;

//-------- Customise the above values --------

char server[] = ORG ".messaging.internetofthings.ibmcloud.com";// Server Name

char publishTopic[] = "iot-2/evt/Data/fmt/json";// topic name and type of event perform and format in which data to be send

char subscribetopic[] = "iot-2/cmd/command/fmt/String";// cmd  REPRESENT command type AND COMMAND IS TEST OF FORMAT STRING

char authMethod[] = "use-token-auth";// authentication method

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;//client id

//-----------------------------------------

WiFiClient wifiClient; // creating the instance for wificlient

PubSubClient client(server, 1883, callback ,wifiClient); //calling the predefined client id by passing parameter like server id,portand wificredential

void setup()// configureing the ESP32

{

**Serial**.begin(115200);

  dht.begin();

  pinMode(LED,OUTPUT);

  delay(10);

**Serial**.println();

  wificonnect();

  mqttconnect();

}

void loop()// Recursive Function

{

  h = dht.readHumidity();

  t = dht.readTemperature();

**Serial**.print("temp:");

**Serial**.println(t);

**Serial**.print("Humid:");

**Serial**.println(h);

  PublishData(t, h);

  delay(1000);

  if (!client.loop()) {

    mqttconnect();

  }

}

/\*.....................................retrieving to Cloud...............................\*/

void PublishData(float temp, float humid) {

  mqttconnect();//function call for connecting to ibm

  /\*

     creating the String in in form JSon to update the data to ibm cloud

  \*/

  String payload = "{\"temp\":";

  payload += temp;

  payload += "," "\"Humid\":";

  payload += humid;

  payload += "}";

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

  if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish ok");// if it sucessfully upload data on the cloud then it will print publish ok in Serial monitor or else it will print publish failed

  } else {

**Serial**.println("Publish failed");

  }

}

void mqttconnect() {

  if (!client.connected()) {

**Serial**.print("Reconnecting client to ");

**Serial**.println(server);

    while (!!!client.connect(clientId, authMethod, token)) {

**Serial**.print(".");

      delay(500);

    }

     initManagedDevice();

**Serial**.println();

  }

}

void wificonnect() //function defination for wificonnect

{

**Serial**.println();

**Serial**.print("Connecting to ");

  WiFi.begin("Wokwi-GUEST", "", 6);//passing the wifi credentials to establish the connection

  while (WiFi.status() != WL\_CONNECTED) {

    delay(500);

**Serial**.print(".");

  }

**Serial**.println("");

**Serial**.println("WiFi connected");

**Serial**.println("IP address: ");

**Serial**.println(WiFi.localIP());

}

void initManagedDevice() {

  if (client.subscribe(subscribetopic)) {

**Serial**.println((subscribetopic));

**Serial**.println("subscribe to cmd OK");

  } else {

**Serial**.println("subscribe to cmd FAILED");

  }

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength)

{

**Serial**.print("callback invoked for topic: ");

**Serial**.println(subscribetopic);

  for (int i = 0; i < payloadLength; i++) {

    //Serial.print((char)payload[i]);

    data3 += (char)payload[i];

  }

**Serial**.println("data: "+ data3);

  if(data3=="lighton")

  {

**Serial**.println(data3);

digitalWrite(LED,HIGH);

  }

  else

  {

**Serial**.println(data3);

digitalWrite(LED,LOW);

  }

data3="";

}